**Section VII**

**TECHNICAL SPECIFICATIONS**

*Procuring Entity: City Government of Tabaco City*

*Contract ID No.: 006-07-2020-GOODS*

*Name of the Project: Supply & Delivery of Two Units Brand New Motorized Fiber Glass Boats*

*Location of the Project: City Agriculture Office, Tabaco City*

***Technical Specifications***

Bidders must state here either “Comply” or any equivalent term in the column “Bidder’s Statement of Compliance” against each of the individual parameters of each “Specification”. Brand of the item offered, if applicable, shall likewise be indicated in the column provided.

|  |  |  |
| --- | --- | --- |
| **Item No.** | **Description** | **Bidder’s Statement of Compliance** |
| 1 | Motorized Fiber Glass Boat |  |
|  | Thickness of Fiber Glass: Bottom: 1inch; Body: ¼ inch |  |
|  | Size: 16m length x 1.5m breadth x 1.2m. depth |  |
|  | Engine: 4D30 Diesel Engine, 4 cylinder; |  |
|  | Displacement: 3298cc; |  |
|  | Bore x stroke: 100 x 105mm, ohv n/a direct injection; |  |
|  | Peak power: 90-95PS (60-70kw) |  |
|  | Inclusive of Accessories: |  |
|  | Anchor, stainless (at least 304) and can hold at least 7 tons of weight |  |
|  | Tadik, made of marurugi |  |
|  | Katig, made of HDPE black pipe, dia=4 inches |  |
|  | 2pcs life vest |  |
|  | 2 pcs life rings |  |
|  | Wooden Paddle (Sagwan) |  |
|  | 50 meters rope 22mm |  |
|  | 17 x 1 ¼ inches Propeller (Elisi), stainless (at least 304) |  |
|  | 1 ¼ inches x 11ft Shafting with support, stainless (at least 304) |  |
|  | 12 x 12x 1 Timon with 1 x 5ft shafting, stainless (at least 304) |  |

I hereby certify to comply with all the above Technical Specifications.

Name of the Company/Bidder Signature over Printed Name Date

of Authorized Representative